### EHV Series

Device | Bit Address | Word Address | Double Word Address | 32 bit | Remarks
--- | --- | --- | --- | --- | ---
External Input | X00000-X05A95 | WX0000-WX05A7 | DX0000-DX05A6 |  | *1 *2
External Output | Y00000-Y05A95 | WY0000-WY05A7 | DY0000-DY05A6 | *2
Remote Input Relay | X10000-X49A95 | WX1000-WX49A7 | DX1000-DX49A6 | *1 *3 *4
Remote Output Relay | Y10000-Y49A95 | WY1000-WY49A7 | DY1000-DY49A6 | *3 *4
Extension External Input | EX00000-EX5A7FF | WEX0000-WEX5A7F | DEX0000-DEX5A7E | *1
Extension External Output | EY00000-EY5A7FF | WEY0000-WEY5A7F | DEY0000-DEY5A7E |
Inner Output | R000-R7BF | - | - |
Data Area | M00000-M7FFFF | WM0000-WM7FFF | DM0000-DM7FFE |
First CPU Link | L00000-L03FFF | WL0000-WL03FF | DL0000-DL03FE |
Second CPU Link | L10000-L13FFF | WL1000-WL13FF | DL1000-DL13FE |
Third CPU Link | L20000-L23FFF | WL2000-WL23FF | DL2000-DL23FE |
Fourth CPU Link | L30000-L33FFF | WL3000-WL33FF | DL3000-DL33FE |
Fifth CPU Link | L40000-L43FFF | WL4000-WL43FF | DL4000-DL43FE |
Sixth CPU Link | L50000-L53FFF | WL5000-WL53FF | DL5000-DL53FE |
Seventh CPU Link | L60000-L63FFF | WL6000-WL63FF | DL6000-DL63FE |
Eighth CPU Link | L70000-L73FFF | WL7000-WL73FF | DL7000-DL73FE |
On Delay Timer | TD0000-TD2559 | - | - |
Off Delay Timer | TDN0000-TDN2559 | - | - |
Single-shot Timer | SS0000-SS2559 | - | - |
Watchdog Timer | WDT0000-WDT2559 | - | - |
Mono Stable Timer | MS0000-MS2559 | - | - |
Retentive Timer | TMR0000-TMR2559 | - | - |
Up-down Counter | CT000-CT511 | - | - |
Up Counter | CU000-CU511 | - | - |
Ring Counter | RCU000-RCU511 | - | - |
Timer Counter (Elapsed Value) | - | TC0000-TC2559 | - |
Word Inner Output | WR00000- WREFFFF | WR0000-WREFFF | DR0000-DREFFE |
Data Area | WN000000-WN1FFFFF | WN00000-WN1FFFF | DN00000-DN1FFFE |

*1Write disable *2Specify as shown below. (Example) External input unit No.1, Slot No.2, Inner Module Bit No.34 (Example) External input unit No.1, Slot No.2, Inner Module Word No.3 *3Specify as shown below. (Example) Remote External Input Remote Master No.1, Remote Slave No.2, Slot No.3, Inner Module Bit No.45 (Example) Remote External Input Remote Master No.1, Remote Slave No.2, Slot No.3, Inner Module Word No.4 *4When using the optical remote communications module, specify as shown below: (Example) Master Station No.1, Slave Station No.2, Slot No.3, Inner Module Bit No.45 (Example) Master Station No.1, Slave Station No.2, Slot No.3, Inner Module Word No.4

#### When using CPU Link

Set the check box of "Use CPU Link" to ON.

When using CPU Link, loop No. and unit No. are added to the address.

(Example) Loop No.1, Unit No.2

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms