### TS series (TS3000/TS3100)

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
External Input Relay | X000 - X07F | X00W - X07W |  | *1
X200 - X27F | X20W - X27W | *2
External Output Relay | Y100 - Y17F | Y10W - Y17W | *1
Y300 - Y37F | Y30W - Y37W | *2
Internal Relay | R000 - R77F | R00W - R27W |
Extended Internal Relay 1 | G000 - G27F | G00W - G27W | *3
Extended Internal Relay 2 | H000 - H27F | H00W - H27W | *4
Edge Relay | E000 - E17F | E00W - E17W |
Latch Relay | L000 - L07F | L00W - L07W |
Timer Relay | T000 - T27F | T00W - T27W |
Counter Relay | C000 - C27F | C00W - C27W |
Special AUX Relay | A000 - A05F | A00W - A05W |
Data Register | ------ | D000 - D27F | *5
------ | D300 - D37F | *6
------ | D400 - D77F | *7
T/C Register 1 | ------ | P000 - P27F |
T/C Register 2 | ------ | V000 - V27F |

*1It is the input signal to the controller. *2It is the output signal to the controller. *3It links the signal input order of the robot program in programmers made by SHIBAURA MACHINE CO., LTD. *4It links the signal output order of the robot program in programmers made by SHIBAURA MACHINE CO., LTD. *5It is data register to be used generally. *6It is data register for backup. *7It is made by SHIBAURA MACHINE CO., LTD. programmer that can be used for robot data acquisition.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms