### Setting of External Device

Use the DIP Switch of the External Device for communication settings of the External Device.

Please refer to the manual of the External Device for more details on settings.

- DIP Switch (SW5)

  DIP Switches | Setting Value | Setup Description
  1 | ON | RS422
  2 | ON | CMP (computer link)
  3 | OFF | Always OFF
  4 | ON | 115.2 Kbps
  5 | OFF | Always OFF
  6 | OFF | Output OFF
  7 | OFF | RUN continuance
  8 | OFF | The scanning is asynchronous.

NOTE

- The following items are fixed.

  Setup Items | Setting Value
  --- | ---
  Data Length | 8 bit
  Stop | 1 bit
  Parity | Even
  Station Number | 0