Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Relay | R000000 - R199915 | R0000 - R1999 |  |
Output Relay |
Internal Auxiliary Relay |
Link Relay | B0000 - B7FFF | B000 - B7FF | *3
Internal Auxiliary Relay | MR000000 - MR399915 | MR0000 - MR3999 |
Latch Relay | LR00000 - LR99915 | LR000 - LR999 |
Control Relay | CR0000 - CR7915 | CR00 - CR79 |
Work Relay | VB0000 - VBF9FF | VB000 - VBF9F | *3
Timer (Contact) | T0000 - T3999 | ------ | - |
Counter (Contact) | C0000 - C3999 | ------ |
Timer (Setting Value) | ------ | TS0000 - TS3999 |  | *1
Counter (Setting Value) | ------ | CS0000 - CS3999 | *1
Timer (Current Value) | ------ | TC0000 - TC3999 | *1
Counter (Current Value) | ------ | CC0000 - CC3999 | *1
Data Memory | ------ | DM00000 - DM65534 |
Extension Data Memory | ------ | EM00000 - EM65534 |
File Register | Current Bank | ------ | FM00000 - FM32767 |
Serial Number System | ------ | ZF000000 - ZF524287 |
Temporary Data Memory | ------ | TM000 - TM511 |
Control Memory | ------ | CM0000 - CM5999 |
Link Register | ------ | W0000 - W7FFF |
Work Memory | ------ | VM00000 - VM50999 |
Index Register | ------ | Z01 - Z12 | *1*2
Digital Trimmer | ------ | TRM0 - TRM7 | *1

*132-bit device

*2Do not write to the addresses Z11 and Z12. They are used in the system of the External Device.

*3The word address descriptions used in the BLUE and the External Device are different. Please be aware of these differences when setting up word addresses.

BLUE | External Device
B000 - B7FF | B0000 - B7FF0
VB000 - VBF9F | VB0000 - VBF9F0

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms