Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) STM6000 (COM1) PC/AT IPC*2 | 14A | RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable + Connector by Phoenix Contact K.K. MC1.5/4-ST-3.5 | Cable length from SIO converter to External Device: 100m or less
14B | RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable + Connector by Phoenix Contact K.K. MC1.5/4-ST-3.5
14C | RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 1 + Junction by AMP 5-1473574-4 + User-created cable 2 + Connector by Phoenix Contact K.K. MC1.5/4-ST-3.5
14D | RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 1 + Junction by AMP 5-1473574-4 + User-created cable 2 + Connector by Phoenix Contact K.K. MC1.5/4-ST-3.5 | Cable length from SIO converter to External Device: 100m or less
GP-4115 (COM1) | 14E | User-created cable + RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable + Connector by Phoenix Contact K.K. MC1.5/4-ST-3.5 | Cable length from SIO converter to External Device: 100m or less
14F | User-created cable + RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable + Connector by Phoenix Contact K.K. MC1.5/4-ST-3.5
14G | User-created cable + RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 1 + Junction by AMP 5-1473574-4 + User-created cable 2 + Connector by Phoenix Contact K.K. MC1.5/4-ST-3.5
14H | User-created cable + RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 1 + Junction by AMP 5-1473574-4 + User-created cable 2 + Connector by Phoenix Contact K.K. MC1.5/4-ST-3.5

*2Only the COM port which can communicate by RS-232C can be used.

IPC COM Port

NOTE

- RS232C conversion unit (RCB-CV-MW) and communication cable (CB-RCA-SIO050) are accessories of PC Interface Software (RCM-101-MW) by IAI Corporation.
- When connecting to 3 or more External Devices, use link connection terminal block or junction by AMP.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.