### CP1E Series

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Channel I/O | 000.00-289.15 | 000-289 |  |
Internal Auxiliary Relay | W00.00-W99.15 | W00-W99 |
Special Auxiliary Relay | A000.00-A753.15 | A000-A753 | *1
Latch Relay | H00.00-H49.15 | H00-H49 |
Timer (Time Up Flag) | T000-T255 | - | *2
Counter (Count Up Flag) | C000-C255 | - | *2
Timer (Current Value) | - | T000-T255 |
Counter (Current Value) | - | C000-C255 |
Data Memory | D0000.00-D8191.15 | D0000-D8191 |

*1Write disable in A000 to A447.

*2Write disable

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms