### FCN/FCJ Series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Coil | 000001 - 009999 | 000001 - 009985 | or *1 |
Discrete Input | 100001 - 109999 | 100001 - 109985 | *2
Input Register | 300001.00 - 309999.15 | 300001 - 309999 | *2
Holding Register | 400001.00 - 409999.15 | 400001 - 409999 |

*1You can set the data storing order in 32-bit data word units and 64-bit data double-word units in the Device Setting dialog box.

*2Write disable

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms