### External Device Settings

Use the programming software (FPWIN GR7S) to set up communication settings on the External Device.

For details on communication settings, please refer to the manual of the External Device.

1. Select the [Create a New Project] option and click [OK].

2. From [Select PLC Type], select the [FP7] option and click [OK].

3. In the project tree, double-click [FP7 configuration].

4. From the [Selection of function] window, select the [Built-in ET-LAN] option and click [OK].

5. From the [Built-in ET-LAN] window, click [Basic communications information].

6. Set the [Home IP address (IPv4)] property to "192.168.1.5".

7. From the [Built-in ET-LAN] window, click [User connection information settings1].

8. Define the External Device setup items with the following values.

   Setup Item | Setting description
   --- | ---
   Connection to use specification | Use
   Connection type | UDP/IP
   Open type (server/client) | Server connection(any destination)
   Open type(automatic/manual) | Open automatically.
   Operating mode setting | MEWTOCOL-7
   Home port number | 60001
   Unused connection disconnect time | 0
   Destination setting method | Specify by IP address (IPv4).
   Destination IP address/name | 192.168.1.1
   Destination port number | 1024

9. Click [OK].

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.