### 5I

1:1

1:n

Legend | Name | Note
--- | --- | ---
(1) | RS-422 terminal block conversion adapter by Pro-face PFXZCBADTM1 |
(2) | User-created cable Connector Display side: Terminal Block External Device side: Terminal Block |

NOTE

- Use the DIP switch in the communication cassette to set the termination resistance. Set SW1-1 of the External Device which terminates the connection to ON.
- Cable length: 1200m or less.