### Setting of External Device

Settings of the External Device vary depending on the connecting port.

##### When using the programmer connector on CPU

Select [PLC System Register Setting] from [Option] of the tool bar in the ladder software to display the [PLC System Register Setting] dialog box. Select the [Tool Port Setting] tab to set as below. Please refer to the manual of the External Device for more details.

Setup Items | Setting Value
--- | ---
Speed | 19200
Data Length | 8
Modem Connection | Disable
Unit No. | 1

##### When using the computer communication unit AFPE224300/AFPE224305/AFPE214325

Select [PLC System Register Setting] from [Option] of the tool bar in the ladder software to display the [PLC System Register Setting] dialog box. Select the [COM Port Setting] tab to set as below. Please refer to the manual of the External Device for more details.

Setup Items | Setting Value
--- | ---
Speed | 19200
Data Length | 8
Parity Setting | Odd
Stop Bit | 1
Operation Selection | Computer link
Modem Connection | OFF
Not automatically change to 2400bps | OFF
Unit No. | 1