Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Relay | R00000 - R59915 | R000 - R599 |  |
Output Relay |
Internal Auxiliary Relay |
Link Relay | B0000 - B1FFF | B000 - B1FF | *6
Internal Auxiliary Relay | MR00000 - MR59915 | MR000 - MR599 |
Latch Relay | LR00000 - LR19915 | LR000 - LR199 |
Control Relay | CR0000 - CR8915 | CR00 - CR89 |
Work Relay | VB0000 - VB1FFF | VB000 - VB1FF | *6
Timer (Contact) | T000 - T511 | ------ | - |
Counter (Contact) | C000 - C255 | ------ |
High-speed Counter Comparator (Contact) | CTC0 - CTC7 | ------ | *1
Timer (Setting Value) | ------ | TS000 - TS511 |  | *2
Counter (Setting Value) | ------ | CS000 - CS255 | *2
Timer (Current Value) | ------ | TC000 - TC511 | *2
Counter (Current Value) | ------ | CC000 - CC255 | *2
Data Memory | ------ | DM00000 - DM32767 |
Temporary Data Memory | ------ | TM000 - TM511 |
Control Memory | ------ | CM0000 - CM8999 |
Link Register | ------ | W0000 - W3FFF |
Work Memory | ------ | VM0000 - VM9499 |
Index Register | ------ | Z01 - Z12 | *2*3
High-speed Counter (Current Value) | ------ | CTH0 - CTH3 | *2*4
High-speed Counter Comparator (Setting Value) | ------ | CTC0 - CTC7 | *2*5

*1Write disable

*232-bit device

*3Do not write to the addresses Z11 and Z12. They are used in the system of the External Device.

*4In the case of KV-NC32T, the maximum value of the address is CTH2. Reading of CTH3 is not a read error, but the value will be 0. If the written, it will write error.

*5In the case of KV-NC32T, the maximum value of the address is CTC5. Reading of CTC6 and CTC7 is not a read error, but the value will be 0. If the written, it will write error.

*6The word address descriptions used in the BLUE and the External Device are different. Please be aware of these differences when setting up word addresses.

BLUE | External Device
B000 - B1FF | B0000 - B1FF0
VB000 - VB1FF | VB0000 - VB1FF0

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms