### 6D

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) SIO converter side: D-Sub 9 pin (socket) |
(2) | SIO converter by IAI Corporation RC*-TU-SIO-* |
(3) | User-created cable Connector SIO converter side TB1: Link connection terminal block TB2: Power supply and emergency stop terminal block Junction side: e-CON connector (plug) |
(4) | Junction by AMP 5-1473574-4 |
(5) | User-created cable Connector Junction side: e-CON connector (plug) Power & I/O Cable side: Terminal block |
(6) | Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB |
(7) | Termination resistance Connector Junction side: e-CON connector (plug) |
(8) | User-created cable Connector Junction side: e-CON connector (plug) |

NOTE

- Cable length from Display to SIO converter: 15m or less
- Cable length from SIO converter to External Device: 100m or less

*1 We recommend the IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB as the Power & I/O Cable.