### MP900/MP2000 Series

Device | Bit address | Word address | 32 bits | Remarks
--- | --- | --- | --- | ---
Enhancing Coil | EGMB000000 - EGMB65534F | EGMB00000 - EGMB65534 |  | *1
Enhancing Input Relay | EGIB00000 - EGIB7FFFF | EGIB0000 - EGIB7FFF | *2
Coil | GMB00000 - GMB4095F | GMB0000 - GMB4095 |
Input Relay | GIB00000 - GIB0FFFF | GIB0000 - GIB0FFF | *2
Input Register | ----- | GIW0000 - GIW7FFF | *2
Holding Register | ----- | GMW00000 - GMW65534 |

*1When you write the bit address, the Display reads the word address corresponding to that of the External Device first. Then, it changes the target bit address among the word data once read and returns the word data to the External Device. Note that the correct data may not be written if you change the word address value in the ladder program while the Display reads the data of the External Device and returns it to the External Device.

*2Write disabled

The Display address is equivalent to the matching External Device address plus the off-set.

The following shows the relationship of addresses between the Display and External Device.

Device | Display on BLUE | Display on External Device
--- | --- | ---
Enhancing Coil (Bit device) | EGMB000000 - EGMB65534F | MW000000+Offset - MW65534F+Offset
Enhancing Coil (Word device) | EGMB00000 - EGMB65534 | MW00000+Offset - MW65534+Offset
Coil (Bit device) | GMB00000 - GMB4095F | MB00000+Offset - MB4095F+Offset
Coil (Word device) | GMB0000 - GMB4095 | MB0000+Offset - MB4095+Offset
Enhancing Input Relay (Bit device) | EGIB00000 - EGIB7FFFF | IW00000+Offset - IW7FFFF+Offset
Enhancing Input Relay (Word device) | EGIB0000 - EGIB7FFF | IW0000+Offset - IW7FFF+Offset
Input Relay (Bit device) | GIB00000 - GIB0FFFF | IB00000+Offset - IB0FFFF+Offset
Input Relay (Word device) | GIB0000 - GIB0FFF | IB0000+Offset - IB0FFF+Offset
Input Register | GIW0000 - GIW7FFF | IW0000+Offset - IW7FFF+Offset
Holding Register | GMW00000 - GMW65534 | MW00000+Offset - MW65534+Offset

e.g) When you specify "GMW00000" in BLUE, the address of "MW00000" to which offset value is added, is specified as the actual address in the External Device. Offset value is described as "Head REG" in the ladder software.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms