### MELSEC Q (Universal model) Series

Device | First 5 digits of the serial No. in the CPU unit: Less than 10042 | First 5 digits of the serial No. in the CPU unit: 10042 or later | 32bits | Notes
--- | --- | --- | --- | ---
Bit Address | Word Address | Bit Address | Word Address
Input Relay | X0000-X1FFF | X0000-X1FF0 | X0000-X1FFF | X0000-X1FF0 |  |
Output Relay | Y0000-Y1FFF | Y0000-Y1FF0 | Y0000-Y1FFF | Y0000-Y1FF0 |
Internal Relay | M00000-M32767 | M00000-M32752 | M00000-M61439 | M00000-M61424 |
Special Relay | SM0000-SM2047 | SM0000-SM2032 | SM0000-SM2047 | SM0000-SM2032 |
Latch Relay | L00000-L32767 | L00000-L32752 | L00000-L32767 | L00000-L32752 |
Annunciator | F00000-F32767 | F00000-F32752 | F00000-F32767 | F00000-F32752 |
Edge Relay | V00000-V32767 | V00000-V32752 | V00000-V32767 | V00000-V32752 |
Step Relay | S0000-S8191 | S0000-S8176 | S00000-S16383 | S00000-S16368 |
Link Relay | B0000-B7FFF | B0000-B7FF0 | B0000-BEFFF | B0000-BEFF0 |
Special Link Relay | SB0000 - SB7FFF | SB0000 - SB7FF0 | SB0000 - SB7FFF | SB0000 - SB7FF0 |
Timer (Contact) | TS00000-TS25023 | - | TS00000-TS32767 | - |
Timer (Coil) | TC00000-TC25023 | - | TC00000-TC32767 | - |
Retentive Timer (Contact) | SS00000-SS25023 | - | SS00000-SS32767 | - |
Retentive Timer (Coil) | SC00000-SC25023 | - | SC00000-SC32767 | - |
Counter (Contact) | CS00000-CS25023 | - | CS00000-CS32767 | - |
Counter (Coil) | CC00000-CC25023 | - | CC00000-CC32767 | - |
Timer (Current Value) | - | TN00000-TN25023 | - | TN00000-TN32767 |
Retentive Timer (Current Value) | - | SN00000-SN25023 | - | SN00000-SN32767 |
Counter (Current Value) | - | CN00000-CN25023 | - | CN00000-CN32767 |
Data Register / External Data Register *1 | - | D00000-D28159 | - | D0000000-D4910079 *2 |
Special Register | - | SD0000-SD2047 | - | SD0000-SD2047 |
Link Register / External Link Register *3 | - | W0000-W6DFF | - | W000000-W4AEBFF *2 |
Special Link Register | - | SW0000-SW6DFF | - | SW0000-SW7FFF |
Module Access Device | - | U000-G00000-U1FF-G65535 | - | U000-G00000-U1FF-G65535 | *5
File Register (Normal) | - | R00000-R32767 | - | R00000-R32767 | *4
File Register (Block switching is not necessary) | - | ZR0000000-ZR4184063 | - | ZR0000000-ZR4849663 | *4
File Register (0R - 31R) | - | 0R0000-0R32767 | - | 0R0000-0R32767 | *4
- | 1R0000-1R32767 | - | 1R0000-1R32767
- | 2R0000-2R32767 | - | 2R0000-2R32767
: | : | : | :
- | 30R0000-30R32767 | - | 30R0000-30R32767
- | 31R0000-31R26623 | - | 31R0000-31R26623

*1External Data Register can be used in the CPU of which first 5 digits of serial No. is 09042 or later.

*2To use addresses D0065536 or higher, or addresses W010000 or higher, the Ethernet interface unit must meet the following requirements:
- The top 5 digits of the serial number are 10042 or later.
- The function version is D or later.

*3External Link Register can be used in the CPU of which first 5 digits of serial No. is 09042 or later.

*4It is different by the memory card which uses the range of file register.

*5This device enables access of the Buffer Memory of SLMP compatible devices or Intelligent Function Modules. The first 3 digits in the address field specify the start I/O number of the intelligent module.

NOTE

- The notation of addresses differs depending on a selected CPU No.
  <Ex.>When 0 is selected for CPU No.,

  <Ex.>When 1 is selected for CPU No.,

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms