### External Device Settings (Ethernet port on basic unit)

Use the programming software (Control Editor) for communication settings. Please refer to the manual of the External Device for more details.

##### Procedure

1. Start the programming software and create the project. The project appears in the offline mode.

2. In the tree view, from [CPU parameters] double-click [CPU settings] and [IP address]. The [CPU Communication Setting (IP Address)] dialog box will appear.

3. Set the items as follows and click [Set].

Setup Items | Setting
--- | ---
IP Address | 192.168.0.1
Subnet mask | 255.255.255.0
Default gateway | 0.0.0.0
Link Speed / Duplex | Auto Negotiation

4. In the tree view, from [CPU parameters] double-click [CPU settings] and [Ethernet (task code)]. The [CPU Communication Setting (Ethernet (task code))] dialog box will appear.

5. Set the port in use as follows, and then click [Set].

Setup Items | Setting | Remarks
--- | --- | ---
Enable | ON |
Number | 3004 | Set a number that is not duplicated on other ports.
Protocol | TCP/IP |
Timeout (sec.) | 30 | Set to 0, when not using timeout.

6. Enter online mode, and transfer the configured settings to the External Device.

7. Restart the External Device.

NOTE

- Check with a network administrator about IP address. Set up unique IP addresses on the same network.
- If you are using a MICRO-EHV series device, select [EHV Series] from the [Series] list in BLUE.