### TCmini series (TC6-00)

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
External Input Relay | Photo coupler | X000 - X00F | X00W - X00W |  | *1
Push-button switch | X100 - X11F | X10W - X11W | *1
External Output Relay | Relay | Y020 - Y02F | Y02W - Y02W | *1
Panel LED | Y160 - Y16F | Y16W - Y16W | *1
External Input Output Relay | X030 - X13F | X03W - X13W | *1
X148 - XF7F | X14W - XF7W | *1
Y030 - Y13F | Y03W - Y13W | *1
Y148 - YF7F | Y14W - YF7W | *1
I000 - IF7F | I00W - IF7W | *1
O000 - OF7F | O00W - OF7W | *1
Internal Relay | R000 - R77F | R00W - R77W | *1
Extended Internal Relay 1 | G000 - GF7F | G00W - GF7W | *1
Extended Internal Relay 2 | H000 - HF7F | H00W - HF7W | *1
Extended Internal Relay 3 | J000 - JF7F | J00W - JF7W | *1
Extended Internal Relay 4 | K000 - KF7F | K00W - KF7W | *1
Edge Relay | E000 - E77F | E00W - E77W | *1
Latch Relay | L000 - L07F | L00W - L07W | *1
Shift Register | S000 - S07F | S00W - S07W | *1
Timer Relay | T000 - T77F | T00W - T77W | *1
Counter Relay | C000 - C77F | C00W - C77W | *1
T/C Register 1 | ------ | P000 - P77F | *1
T/C Register 2 | ------ | V000 - V77F | *1
Generic Register 1 | ------ | D000- DF7F | *1
Generic Register 2 | ------ | B000- BF7F | *1
Generic Register 3 | ------ | U000- UF7F | *1
Generic Register 4 | ------ | M000- MF7F | *1
Generic Register 5 | ------ | Q000- QF7F | *1

*1Device format is as follows: Please refer to the manual of External Device for more detail.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms