### External Device Settings

Use the ENI/ENIW Utility for communication setting.

Please refer to the ENI/ENIW Utility manual for more details.

1. Start up the ENI/ENIW Utility.

2. Use the [ENI IP Addr] tab to set IP address and other items.

3. Download the settings in 1761-NET-ENI and restart the External Device.

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.

NOTE

- The device storage order of data varies depending on the External Device. Change the String Mode to match the device order same as a External Device.