Display (Connection Port) | Cable | Notes
--- | --- | ---
GP-4116 (COM1) | 4E | User-created cable | Cable length: 500m or less
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*c-2 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 4F | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 + User-created cable | Cable length: 500m or less
4A | COM port conversion adapter by Pro-face CA3-ADPCOM-01 + Connector terminal block conversion adapter by Pro-face CA3-ADPTRM-01 + User-created cable
4B | User-created cable
PS5000 PS6000 (Optional Interface) PSA6000 *3 | 4G | User-created cable | Cable length: 500m or less

*c-2Except ST-6200

*3Available only with COM ports that support RS-422/485 (4wire).

IPC COM Port

IMPORTANT:

- Terminal number to be used for communication varies depending on the External Device. Terminal numbers corresponding to each series are shown below.

  Pin | KV-L20V KV-L21V | KV-N11L KV-NC20L
  --- | --- | ---
  SDB(+) | 5 | 2
  SDA(-) | 3 | 1
  RDB(+) | 4 | 4
  RDA(-) | 2 | 3
  SG | 1 | 5

#

NOTE

- Set the PORT2 toggle switch on the External Device to "422A 485(4)". Also, turn ON the switch of the terminator.

- Pay attention that pole A and pole B are reversely named for the Display and the External Device.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.