### 4G)

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block External Device side: Uni-Telway connection cable |
(2) | Uni-Telway cable by Schneider Electric Industries TSX SCP CU 4030 (3m) |

NOTE

- Cable length: 10m or less.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON