Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
External input relay | X0000 - X109F | WX000 - WX109 |  |
External output relay | Y0000 - Y109F | WY000 - WY109 |
Link relay | L0000 - L127F | WL000 - WL127 |
Internal relay | R0000 - R511F | WR000 - WR511 |
Special internal relay | R9000 - R951F | WR900 - WR951 | *1
Data register | - | DT00000 - DT65532 |
Link data register | - | LD000 - LD255 |
Timer elapsed value register | - | EV0000 - EV1023 |
Timer(Contact) | T0000 - T1023 | - | *1
Counter elapsed value register | - | EV0000 - EV1023 |
Counter(Contact) | C0000 - C1023 | - | *1
Special data register (DT) | - | DT90000 - DT90999 | *1
Timer set value register | - | SV0000 - SV1023 |
Counter set value register | - | SV0000 - SV1023 |

*1Write disabled

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms