### 9G

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable • Connector Display side: Terminal block External Device side: Terminal block |

NOTE

- Please set the terminating resistor switch to the "100Ω" position only on the last External Device in the chain.

NOTE

- Total cable length: 500m or less

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON