### Settings of External Device

Communication setting of CPU module by ladder software. (Check the operation in MPE720 Ver.7)

Refer to your External Device manual for communication setting details.

#### Ladder Software Setting

1. Start up the ladder software.

2. Create a project.

3. From the [System] menu, select [Module constitution].

4. Click [Detail] for the corresponding link I/F you want to use.

5. In the dialog box, configure the following settings.

   Setup Items | Setup Description
   --- | ---
   Transmission parameter | IP address | 192.168.0.1 (External Device IP address)
   Connection parameter (Connection number 1) | My Port | 1024 (External Device port number)
   DST. IP Address | 192.168.0.10 (Display's IP address)
   DST. Port | 1024 (Display's port number)
   Connection type | UDP
   Protocol type | Expansion memobus
   Code | BIN

6. Double-click [Setting] to open the [Detail settings] dialog box.

7. Set [Automatically Reception] to the [Enable] option and click [OK].

8. Save and download the communication settings to the External Device.

#####

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.
- When [Automatically Reception] is disabled, you need to set up a ladder program for communication.

"Ladder Program for Communication"

##### Ladder Program for Communication