### External Device Settings

Use RSLogix500 for communication setting.

Please refer to the manual of RSLogix500 for more details.

1. Start up RSLogix500 and create a new project. Select the CPU to be used when creating a new project.

2. Select [Channel Configuration] from [Controller] in the displayed Project tree.

3. Select [Open] from the menu displayed by right-clicking [Channel Configuration] and display the Channel setting screen.

4. Use the [Chan.1 - System] tab to set IP address and other items.

5. Download the setting in the External Device and restart the External Device.

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.

NOTE

- The device storage order of data varies depending on the External Device. Change the String Mode to match the device order same as a External Device.

NOTE

- Rockwell EtherNet/IP driver for Display uses the CIP protocol. Old revision of SLC 5/05 CPU does not support it. Upgrade CPU Series A to the firmware revis501, FRN5 or later. CPU Series B and C support the CIP protocol.