### Setting of External Device

Use Shenzhen Inovance technology’s setting tool (AutoShop) to configure communication settings on the External Device.

Refer to your External Device manual for details.

1. Start up the setting tool.

2. From the [Tools] menu, select [Communication Setting].

3. Click [Change IP].

4. In the [New IP Address] field enter "192.168.0.1" and click [Change IP].

5. When a message appears declaring the IP address has changed, click [OK].

6. In the [Subnet mask] field enter "255.255.255.0".

NOTE

- Check with a network administrator about IP address.
  Do not set the duplicate IP address.