### PXG series

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Read Only Bit Data | 10001 - 10013 | - |  | *1
Read Only Word Data (Internal) | - | 30001 - 30062 | *1
Read Only Word Data (Engineering Unit) | - | 31001 - 31062 | *1
Word Data (Internal) | 40002.00 - 40628.15 | 40002 - 40628 | *2
Word Data (Engineering Unit) | 41002.00 - 41628.15 | 41002 - 41628 | *2

*1Write disabled.

*2When you write to the bit address, the Display reads the entire word, sets the defined bit, then returns the new word value to the External Device. If the ladder program writes data to this word address during the bit write process, the resulting data may be incorrect.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms