### 4E)

No. | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block External Device side: Half-pitch 20pin (Plug) (JD40) |

NOTE

- Cable length: 1200m or less.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON