### Settings of External Device

Use the LS ELECTRIC programming tool (XG5000) to define External Device communication settings.

Refer to your External Device manual for details.

1. Start up the configuration tool.

2. From the [Project] menu, select [New Project].

3. Configure the [PLC Series] and [CPU type], and click [OK].

4. In the tree view, right-click [Network Configuration] - [Undefined Network] and add the communication module.

5. Set the link interface you are using.

6. From the tree view, double-click the added link interface to display the [Standard Settings] dialog box.

7. Set the [Standard Settings] properties as follows, and click [OK].

Setup Items | Setup Description
--- | ---
IP Address | 192.168.0.1
Subnet mask | 255.255.255.0
Gateway | 192.168.0.1
Server Mode | XGT server

5. From the [Online] menu, select [Write] .

6. Select the External Device, and click [OK].

7. Restart the External Device.

NOTE

- Check with a network administrator about IP address.
  Do not set the duplicate IP address.