### External Device Settings

For External Device communication settings, use the Station No. Configuration switch on the front of the controller.

Refer to your External Device manual for details.

1. Set "0" to Station No. Configuration switch.

   NOTE

   - The Station Number is generated by adding 1 (one) to the value set by the Station No. Configuration switch.

Other communication settings are fixed as below.

Setting Items | Setting Value
--- | ---
Communication speed | 19200
Data length | 8
Stop bit | 1
Parity | None