### Settings of External Device

Set PC No. of the External Device using DIP Switches and the rotary switch of External Device.

Please refer to the manual of the External Device for more details.

After setting, reboot the External Device to enable the setting.

##### Setup Items

- DIP Switch

DIP Switch | Settings*1 | Setup Description
--- | --- | ---
SW1 | OFF | Set PC No. by combining with the rotary switch.
SW2 | OFF
SW3 | ON | Link Master
SW4 | OFF | Link Slave
SW5 | OFF | Remote Master
SW6 | OFF | Remote Slave

*1For SW3 to SW6, if two or more than two switches are turned on, there will be a set error.
Turn on SW3 when you connect to Display.

- Rotary switch

Settings | Setup Description
--- | ---
0 | PC No.

NOTE

- Set PC No. using DIP Switches 1 and 2 and the rotary switch. Combination of possible settings is as follows.

  DIP Switch | PC No. that can be set with the rotary switch
  SW1 | SW2
  OFF | OFF | 0 - 15
  OFF | ON | 16 - 31
  ON | OFF | 32 - 47
  ON | ON | 48 - 63