### 5A

No. | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: D-sub 9 pin (socket) External Device side: D-sub 9 pin (socket) | Instead of connecting the Display (FG), connect the Shield to the Shell.
(2) | AIC+ Advanced Inter face Converter by Rockwell Automation, Inc. 1761-NET-AIC |
(3) | RS-232C cable by Rockwell Automation, Inc. 1761-CBL-AM00 |

NOTE

- Cable length: 15m or less.