# Error Detection (FS Error)

When a protocol error occurs, this command allows the Display or the Host to output an error notice about the other unit/device.

This frame does not require a response.

Host: Command Data

- Inter-character timeout error frame

Data Name

- Data: "Error Receive time out"

- Display presence monitoring timeout error frame

Data Name

- Data: "Error Alive time out"

- Inter-protocol timeout error frame

Data Name

- Data: "Error Response time out"

Display: Response Data

- Inter-character timeout error frame

Data Name

- Data: "Error Receive time out"

- Display presence monitoring timeout error frame

Data Name

- Data: "Error Alive time out"

- Inter-protocol timeout error frame

Data Name

- Data: "Error Receive time out"