### MP900/2000/CP-9200SH

Device | Display on BLUE | Supported Address*1 | 32 bits | Remarks
--- | --- | --- | --- | ---
Enhancing Coil (Bit device) | EGMB000000-EGMB65534F | MW000000 + Offset -MW65534F + Offset |  | *2
Enhancing Coil (Word device) | EGMB00000-EGMB65534 | MW00000 + Offset -MW65534 + Offset |
Enhancing Input Relay (Bit device) | EGIB00000-EGIB7FFFF | IW00000 + Offset - IW7FFFF + Offset | *3
Enhancing Input Relay (Word device) | EGIB0000-EGIB7FFF | IW0000 + Offset - IW7FFF +Offset | *3
Coil (Bit device) | GMB0000.0-GMB4095.F | MW00000 + Offset - MW4095F + Offset |
Coil (Word device) | GMB0000-GMB4095 | MW0000 + Offset - MW4095 + Offset |
Input Relay (Bit device) | GIB0000.0-GIB0FFF.F | IW00000 + Offset - IWOFFFF + Offset | *3
Input Relay (Word device) | GIB0000-GIB0FFFF | IW0000 + Offset - IW0FFFF + Offset | *3
Input Register | GIW0000-GIW7FFF | IW0000 + Offset - IW7FFFF + Offset | *3
Holding Register | GMW00000-GMW65534 | MW00000 + Offset - MW65534 + Offset |

*1When you specify "GMW00000" in BLUE, the address of "MW00000" to which offset value is added, is specified as the actual address in the External Device. Offset value is described as "Head REG" in the ladder software.

*2When you write the bit address, the Display reads the word address corresponding to that of the External Device first. Then, it changes the target bit address among the word data once read and returns the word data to the External Device. Note that the correct data may not be written if you change the word address value in the ladder program while the Display reads the data of the External Device and returns it to the External Device.

*3Write disable

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms