### Setting of External Device

Set the computer link module as below.

Please refer to the manual of the External Device for more details on settings.

Setup Items | Settings
Speed | 19200bps
Data Bit | 8bit
Stop Bit | 1bit
Parity Bit | Even
RS422 Connecting Port*1 | 2wire
STATION No. | 0

*1When using PC/CMP-LINK (THU-2755), only 2-wire type is available to use. In addition, when using PC3J command, the link unit in ver. 5.00 or higher is required.

NOTE

- To communicate PC/CMP-LINK (THU-2755) and PC3JD/PC3JG using PC3J command, use the link unit ver. 5.00 or later is required. Also, the link unit does not have the settings of PC2J or PC3J selection switch (SW) etc. Error occurs when sending PC3J command to the link unit in less than ver. 5.00.