### RS-422 (2-wire) connection

Display (Connection Port) | Cable | Remarks
--- | --- | ---
GP-4116 (COM1) | 3G | User-created cable | Cable length: 1000m or less.
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 3A | COM port conversion adapter by Pro-face CA3-ADPCOM-01 + Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 + User-created cable | Cable length: 1000m or less.
3I | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 + User-created cable
3B | User-created cable
PS5000 PS6000 (Optional Interface) PSA6000 *8 | 3K | User-created cable | Cable length: 1000m or less.

*b-3Except ST-6200

*8Only the COM port which can communicate by RS-422/485 (2 wire) can be used.

IPC COM Port

NOTE

- Control method when using the RS422 cable is XON/XOFF only. XON/XOFF control is enabled only for ASCII.

Forced:

1. - Use the twist pair cable with approx. 50pF/m capacitance, 100Ω characteristic impedance, made of 24AWG rod.

IMPORTANT:

- The RS422 cable length is normally 1000m at maximum, but the cable length has the limit depending on the connecting host device. For connection, be sure to refer to the manual of the connecting host device.
- The connecting method or termination resistance varies depending on the connecting host device. Connect SG if provided.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.