Device | Bit Address | Word Address | 32bits | Remarks
--- | --- | --- | --- | ---
Input / Output Relay | P00000 - P2047F | P0000 - P2047 |  |
Auxiliary Relay | M00000 - M2047F | M0000 - M2047 |
Keep Relay | K00000 - K4095F | K0000 - K4095 | *1
Link Relay | L000000 - L11263F | L00000 - L11263 |
Special Relay | F00000 - F2047F | F0000 - F2047 | *2
Timer (Contact) | T0000 - T2047 | ------ |
Counter (Contact) | C0000 - C2047 | ------ |
Timer (Current Value) | ------ | T0000 - T2047 |
Counter (Current Value) | ------ | C0000 - C2047 |
Data Register | ------ | D00000 - D32767 |
Special Module Register | ------ | U00.00 - U7F.31 | *3
Index Register | ------ | Z000 - Z127 |
Communication Data Register | ------ | N00000 - N21503 |
File Register | ------ | R00000 - R32767 | *4
File Register | ------ | ZR00000 - ZR65535 | *4

*1 If the CPU is XGK, the bit address is "K00000 - K2047F" and the word address is "K0000 - K2047".

*2 Write disable

*3 The feature of U Device is like this:

*4 XBM does not support the File Register.

XBC supports only File Register R. (File Register R and ZR are the same device in the XBC.)

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms