Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Relay | 00000 - 59915 | 000 - 599 |  | *1
Output Relay | *1
Internal Auxiliary Relay | *1
Internal Auxiliary Relay | MR00000 - MR99915 | MR000 - MR999 |
Latch Relay | LR00000 - LR99915 | LR000 - LR999 |
Control Relay | CR0000 - CR3915 | CR00 - CR39 |
Timer (Contact) | T0000 - T3999 | ------ | - |
Counter (Contact) | C0000 - C3999 | ------ |
High-speed Counter Comparator (Contact) | CTC0 - CTC3 | ------ | *2
Timer (Setting Value) | ------ | TS0000 - TS3999 |  | *3
Counter (Setting Value) | ------ | CS0000 - CS3999 | *3
Timer (Current Value) | ------ | TC0000 - TC3999 | *3
Counter (Current Value) | ------ | CC0000 - CC3999 | *3
Data Memory | ------ | DM00000 - DM65534 |
Extension Data Memory EM | ------ | EM00000 - EM65534 |
Extension Data Memory FM | ------ | FM00000 - FM32766 |
Temporary Data Memory | ------ | TM000 - TM511 |
Control Memory | ------ | CM00000 - CM11998 |
Index Register | ------ | Z01 - Z12 | *4
Digital Trimmer | ------ | TRM0 - TRM7 | *3
High-speed Counter (Current Value) | ------ | CTH0 - CTH1 | *3
High-speed Counter Comparator (Setting Value) | ------ | CTC0 - CTC3 | *3

*1R000 to R599 (R00000 to R59915) are shown in KV-1000, but 000 to 599 (00000 to 59915) in BLUE.

*2Write disable

*332-bit device

*4Do not write to the addresses Z11 and Z12. They are used in the system of the External Device.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms