### Settings of External Device (EH-ETH)

Use the Web Browser to access the Ethernet unit for communication setting.
Note that the ladder software (Ladder Editor for Windows) is used for setting up the environment of the External Device.

Please refer to the manual of the EH-ETH for more details.

1. Assign the Ethernet unit to CPU unit by using [I/O assign] in the ladder software.

2. Turn ON the DIP Switch 1 and 6 of the Ethernet unit, and turn ON the power. Then, a temporary address (192.168.0.4) for accessing the Ethernet unit will be set.

Bit No.*1 | Operation Mode
1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
ON | OFF | OFF | OFF | OFF | ON | OFF | OFF | Ethernet Information Setting Mode

*1Use Bit No.3 to No.8 to set the fourth octet of IP address. The IP address is fixed to 192.168.0. until the third octet.

3. Connect the PC’s Ethernet port and the EH-ETH’s Ethernet port by LAN cable. (Connect via HUB or connect directly using a cross cable.)

4. Enter "http://192.168.0.4/" in the address input box of the Web Browser to access the Ethernet unit.

IMPORTANT:

- To access, PC’s IP address up to the third octet must be set to 192.168.0. (192.168.0.10, etc.)

5. Select [IP Address] from the menu frame in the displayed screen and set IP address.

6. Similarly, select [Task Code] from the menu frame and set [Port No.] and [Protocol].
Also, please set the IP Address, [Port No.] and [Protocol] as the same value as those set on the Display side.

7. Turn OFF the power of the External Device. After turning OFF all DIP Switches, turn ON the power of the External Device.

NOTE

- Check with a network administrator about IP address. Set up unique IP addresses on the same network.

NOTE

- When connecting with Display, EH-ETH with SOFTWARE VER.06 or later is required. (Check the label of EH-ETH main body for the version.)