### External Device Settings

Use the ladder software (Logic Designer) for communication settings. Refer to your External Device manual for details.

1. Start up the ladder software.

2. To start the MODBUS communication (RTU mode) slave function, create the control logic. For the example of control logic, refer to "Control Logic Example".

   Control Logic Example

3. Select [Rebuild Project] from the [Build] menu.

4. Double-click [Target Setting] in the project tree Window to display the [Target] dialog box.

5. Enter "192.168.0.1" in [Host Name/IP Address].

6. Click [OK].

7. Download the communication settings to the External Device.

8. Reboot the External Device.

##### Control Logic Example

To connect the Display to the External Device, the control logic is required.

The control logic example is shown below.

NOTE

- Check with the network administrator about the IP address. Do not duplicate IP addresses.
- Please refer to the manual of the ladder software for details on other settings.

- Use an integer from 0 to 247 and 255 to enter the unit ID of the External Device.