Display (Connection Port) | Cable | Notes
--- | --- | ---
GP-4116 (COM1) | 4G | User-created cable + Uni-Telway cable by Schneider Electric Industries TSX SCP CU 4030 (3m) | The cable length have to be 10m or less. For n:1 connection, you need user-created cable for connection between the s.
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 4I | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 + Uni-Telway connection cable TSX SCP CU 4030 (3m) by Schneider Electric Industries | Cable length: 10m or less. For n:1 connection, you need user-created cable for connection between the Displays.
4A | COM Port Conversion Adapter by Pro-face CA3-ADPCOM-01 + Terminal Block Conversion Adapter by Pro-face CA3-ADPTRM-01 + User-created cable + Uni-Telway connection cable by Schneider Electric Industries TSX SCP CU 4030 (3m)
4B | User-created cable + Uni-Telway cable by Schneider Electric Industries TSX SCP CU 4030 (3m)
PS5000 PS6000 (Optional Interface) PSA6000 *8 | 4K | User-created cable + Uni-Telway cable by Schneider Electric Industries TSX SCP CU 4030 (3m) | Cable length: 10m or less. For n:1 connection, you need user-created cable for connection between the Displays.

*b-3Except ST-6200

*8Only the COM port which can communicate by RS-422/485 (2 wire) can be used.

IPC COM Port

NOTE

- Line color for both D (A) and SG is white. As SG (red) and SG (white) are twisted pair, as well as D (A) and D (B), you can judge which line is SG or D (A).

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.