### 4B

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) External Device side: D-Sub 15 pin (plug) | Instead of connecting the Display (FG), connect the Shield to the Shell.
(2) | Conversion cable by Hitachi IES Co., Ltd. EH-RS05 |

NOTE

- Cable length: 500m or less
- For more information about the termination resistance, contact Hitachi IES Co., Ltd.