### Settings of External Device

Use the rotary switch of Ethernet port on CPU unit and the ladder software SX-Programmer Expert (D300win) for communication settings.

Please refer to the Micrex-SX Series D300Win users manual by Fuji Electric Co., Ltd. for more details.

##### Rotary Switch Settings

Set "0" to the rotary switch of Ethernet port on CPU

##### Ladder Software Setting

1. Start up the D300win.

2. Select [New Project] from the [File] menu and select template of using CPU from the New Project dialog.

3. Double click [System Definition] of the project tree to display the system definition screen.

4. Select [Properties] from the displayed menu indicated after right-clicking the CPU.

5. Click [Parameter] of the [Module properties] dialog box.

6. Select [IP Address/Gateway Setting] tub of [CPU Parameter] dialog box.

7. Input IP address and subnet mask as shown below in [IP Address/Gateway Setting].

   Setup Items | Setup Description
   --- | ---
   IP Address | 192.168.0.1
   Subnet mask | 255.255.255.0

8. Select [Detail Setting] of [IP Address/Gateway Setting] tub.

9. Select [Self port standard No.] and input "773" to the port number of Ethernet port above CPU unit.

NOTE

- For the port number of Device Setting for BLUE, set the value that "251" is added to the set port number.
  For example, if "773" is set to the port number, set "1024" to the port number of Device Setting for BLUE.

10. Select [Exit] from [File] menu on the system definition screen.

11. Select [Make] from [Build] menu and compile the project.

12. Select [Project Control] from [Online] menu and click [Download].

13. Select all items to be downloaded and click [OK].

14. After download is executed normally, click [Reset].

Now communication setting is completed.

NOTE

- When using the SPH5000M series, in the driver properties, select [SPH5000M] for the [CPU Series].