### PC3J, PC3JD, PC3JG, PC3JT

Device | Bit Address | Word Address | 32bits | Remarks
--- | --- | --- | --- | ---
Input Relay | 1X0000 - 1X07FF | 1X000W - 1X07FW |  | *2 *3
2X0000 - 2X07FF | 2X000W - 2X07FW
3X0000 - 3X07FF | 3X000W - 3X07FW
Output Relay | 1Y0000 - 1Y07FF | 1Y000W - 1Y07FW | *2 *3
2Y0000 - 2Y07FF | 2Y000W - 2Y07FW
3Y0000 - 3Y07FF | 3Y000W - 3Y07FW
Internal Relay | 1M0000 - 1M07FF | 1M000W - 1M07FW | *2
2M0000 - 2M07FF | 2M000W - 2M07FW
3M0000 - 3M07FF | 3M000W - 3M07FW
Keep Relay | 1K0000 - 1K02FF | 1K000W - 1K02FW | *2
2K0000 - 2K02FF | 2K000W - 2K02FW
3K0000 - 3K02FF | 3K000W - 3K02FW
Link Relay | 1L0000 - 1L07FF | 1L000W - 1L07FW | *2
2L0000 - 2L07FF | 2L000W - 2L07FW
3L0000 - 3L07FF | 3L000W - 3L07FW
Special Relay | 1V0000 - 1V00FF | 1V000W - 1V00FW | *2
2V0000 - 2V00FF | 2V000W - 2V00FW
3V0000 - 3V00FF | 3V000W - 3V00FW
Edge Detection | 1P0000 - 1P01FF | ------ |
2P0000 - 2P01FF | ------
3P0000 - 3P01FF | ------
Timer (Contact) | 1T0000 - 1T01FF | 1T000W - 1T01FW | *2 *3
2T0000 - 2T01FF | 2T000W - 2T01FW
3T0000 - 3T01FF | 3T000W - 3T01FW
Counter (Contact) | 1C0000 - 1C01FF | 1C000W - 1C01FW | *2 *3
2C0000 - 2C01FF | 2C000W - 2C01FW
3C0000 - 3C01FF | 3C000W - 3C01FW
Present Value Register | 1N0000-0 - 1N01FF-F | 1N0000 - 1N01FF | *4
2N0000-0 - 2N01FF-F | 2N0000 - 2N01FF
3N0000-0 - 3N01FF-F | 3N0000 - 3N01FF
Data Register | 1D0000-0 - 1D2FFF-F | 1D0000 - 1D2FFF *5 | *4
2D0000-0 - 2D2FFF-F | 2D0000 - 2D2FFF *5
3D0000-0 - 3D2FFF-F | 3D0000 - 3D2FFF*5
Link Register | 1R0000-0 - 1R07FF-F | 1R0000 - 1R07FF | *4
2R0000-0 - 2R07FF-F | 2R0000 - 2R07FF
3R0000-0 - 3R07FF-F | 3R0000 - 3R07FF
Special Register | 1S0000-0 - 1S03FF-F | 1S0000 - 1S03FF | *4
2S0000-0 - 2S03FF-F | 2S0000 - 2S03FF
3S0000-0 - 3S03FF-F | 3S0000 - 3S03FF
File Register | B0000-0 - B1FFF-F | B0000 - B1FFF | *4
Extension Input | EX0000 - EX07FF | EX000W - EX07FW | *2 *3
Extension Output | EY0000 - EY07FF | EX000W - EY07FW | *2 *3
Extension Internal Relay | EM0000 - EM1FFF | EM000W - EM1FFW | *2
Extension Special Relay | EV0000 - EV0FFF | EV000W - EV0FFW | *2
Extension Keep Relay | EK0000 - EK0FFF | EK000W - EK0FFW | *2
Extension Edge Detection | EP0000 - EP0FFF | ------ |
Extension Timer | ET0000 - ET07FF | ET000W - ET07FW | *2 *3
Extension Counter | EC0000 - EC07FF | EC000W - EC07FW | *2 *3
Extension Link Relay | EL0000 - EL1FFF | EL000W - EL1FFW | *2
Extension 2 Input | GX0000 - GXFFFF | GX000W - GXFFFW | *2 *3 *6
Extension 2 Output | GY0000 - GYFFFF | GY000W - GYFFFW | *2 *3 *6
Extension 2 Internal Relay | GM0000 - GMFFFF | GM000W - GMFFFW | *2 *6
Extension Data Register | U0000-0 - U7FFF-F | U0000 - U7FFF | *4
Extension Setting Value Register | H0000-0 - H07FF-F | H0000 - H07FF | *4
Extension Special Register | ES0000-0 - ES07FF-F | ES0000 - ES07FF | *4
Extension Current Value Register | EN0000-0 - EN07FF-F | EN0000 - EN07FF | *4
Watch Time Register | ------ | WT0 - WT6 | *7 *8
Extended buffer register | EB00000-0 - EB1FFFF-F | EB00000 - EB1FFFF | *4

*2For word description of BitDevice, add "W" to the last of the word address.
Example) When the address is 0 in M device, describe "M0000W".

*3You cannot set the duplicate address for X and Y (EX, EY, GX, GY), T and C (ET, EC).
(Setting such address as X000/Y000, EX000/EY000, T000/C000, ET000/EC000 is wrong.)

*4For bit description of WordDevice, describe "-" following the word address and the bit position next.
Example) When the address is 0 and the bit is 5 in D device, describe "D0000-5".

*5Maximum address value of PC3J and PC3JT is 2FFF, and of PC3JD and PC3JG is 0FFF.

*6Supported by Link I/F on the CPU of PC3JG.

*7When you write "Watch Time Register", the Display reads all addresses of "Watch Time Register" in the External Device. Then the Display writes all addresses of "Watch Time Register" after the Display changes the data of your requested address. Note that the correct data may not be written if you change the word address using the ladder program while the Display reads data from the External Device and returns it.

*8Contents of "Watch Time Register" are shown below.

Address | Mean | Note
WT0 | day of week | 0:Sunday, 1:Monday, 2:Tuesday, 3:Wednesday, 4:Thursday, 5:Friday, 6:Saturday
WT1 | year | lower two digits of A.D.
WT2 | month |
WT3 | day |
WT4 | hour | 24-hour system
WT5 | minute |
WT6 | second |

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms