### 18G

1:1

1:n

Legend | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block External Device: Terminal block |

NOTE

- Use the termination resistance selector switch in the communication cassette to set the termination resistance. Set termination resistance selector switch of the External Device which terminates the connection to ON.
- Cable length: 1200m or less.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON