### Settings of External Device

Use the ladder software "RSLogix 500" for communication settings.

Open "Channel Configuration" of "RSLogix 500" to perform the settings in the "Chan. 0 - System" tab.

##### For Full Duplex

Setup Items | Setup Description
--- | ---
Driver | DF1 Full Duplex
Baud | 19200
Parity | NONE
Stop Bits | 1
Control Line | No Handshaking
Error Detection | CRC
Embedded Responses | Auto-detect
Duplicate Packet Detect | Disabled
ACK Timeout | 50
NAK Retries | 3
ENQ Retries | 3
Source ID | 0

##### For Half Duplex

Setup Items | Setup Description
--- | ---
Driver | DF1 Half Duplex Slave
Baud | 19200
Parity | NONE
Stop Bits | 1
Control Line | No Handshaking
Error Detection | CRC
EOT Suppression | Disabled
Duplicate Packet Detect | Disabled
Poll Timeout | 3000
Message Retries | 3
Pre Transmit Delay | 0
Node Address | 0

NOTE

- Please refer to the manual of the ladder software for more detail on other setting description.