Device | Bit Address | WordAddress | 32bits | Notes
--- | --- | --- | --- | ---
Parameter*1 | 000.00 - 991.15 | 000 - 991 |  | *2 *3
000.00 - 993.15 | 000 - 993
Parameter*4 | P037.00 - P037.31 | P037 | - | *3 *5
Setting Items and Set Data*6 | S00.00 - S59.15 | S00 - S59 |  | *3 *7 *8
Setting Items and Set Data*9 | SL00.00 - SL59.31 | SL00 - SL59 | - | *3 *7 *8

*1Exception is parameter 37 of FR-E500 series, FR-S500 series, FR-F500J series, and FR-E700 series. *2The range, "000 to 993", can be used for the External Device of FR-C500 series, FR-S500 series, and FR-F500J series. *3When you write to the bit address, the Display reads the entire word, sets the defined bit, then returns the new word value to the External Device. If the ladder program writes data to this word address during the bit write process, the resulting data may be incorrect. *4Parameter 37 of FR-E500 series, FR-S500 series, FR-F500J series, and FR-E700 series. *5Specify "P037" (32 bit External Device) for Parameter 37 of FR-E500 series, FR-S500 series, FR-F500J series, and FR-E700 series. When "037" is used, an unexpected error occurs. *6Setting items and set data of the series except for FR-V500/FR-V500L series. *7Setting item differs depending on the series. Check for the setting item list before reading or writing a setting item. *8There are some items that are only for reading or writing among the setting items. Refer to the table below before reading/writing a setting item.
Setting Items | Read/Write
--- | ---
S01 to S04, S06 to S46, S49 to S52 SL01 to SL04, SL06 to SL46, SL49 to SL52 | Read only
S47 to S48, S53 to S57 SL47 to SL48, SL53 to SL57 | Write only*A
S00, S05, S58 to S59 SL00, SL05, SL58 to SL59 | Read and Write
*A Use word write operations when writing data. Using a bit write operation causes an error. *9Setting items and set data of the FR-E500 series, FR-S500 series, FR-F500J series, FR-E700 series and FR-V500/FR-V500L.