### TCmini series (TC9-00)

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
External Input Relay | Contact Input | X000 - X007 | X00W - X00W |  | *1
DIP Switch | X008 - X009 | *1
Key Switch | X100 - X10F | X10W - X10W | *1
External Output Relay | Transistor | Y020 - Y027 | Y00W - Y00W | *1
LED | Y140 - Y147 | Y14W - Y14W | *1
Internal Relay | X000 - X17F Y000 - Y17F R000 - R37F | X00W - X17W Y00W - Y17W R00W - R37W | *1 *2
Edge Relay | E000 - E07F | E00W - E07W | *1
Latch Relay | L000 - L03F | L00W - L03W | *1
Timer Relay | T000 - T13F | T00W - T13W | *1
Counter Relay | C000 - C13F | C00W - C13W | *1
Special AUX Relay | A000 - A15F | A00W - A15W | *1
Data Register | ------ | D000 - D27F | *1
T/C Register 1 | ------ | P000 - P13F | *1
T/C Register 2 | ------ | V000 - V13F | *1

*1Device format is as follows: Please refer to the manual of the External Device for more details. *2Results from External Input Relay or External Output Relay are given priority for areas mapped to External Input Relay or External Output Relay.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms