### CP2E Series

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Channel I/O | 000.00-289.15 | 000-289 |  |
Internal Auxiliary Relay | W000.00-W127.15 | W000-W127 |
Special Auxiliary Relay | A000.00-A959.15 | A000-A959 | *1
Latch Relay | H000.00-H127.15 | H000-H127 |
Timer (Time Up Flag) | T000-T255 | - | *2
Counter (Count Up Flag) | C000-C255 | - | *2
Timer (Current Value) | - | T000-T255 |
Counter (Current Value) | - | C000-C255 |
Data Memory | D00000.00-D16383.15 | D00000-D16383 |
Index Register | - | IR00-IR15 | *3
Data Register | - | DR00-DR15 | *3

*1Write disable in A000 to A447.

*2Write disable

*3You cannot write during RUN.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms