### Millenium 3

Device | Bit Address | Word Address | 16 bits | 32 bits | Notes
--- | --- | --- | --- | --- | ---
SL IN | SL IN 1 - BIT1 to SL IN 24 - BIT16 | SL IN 1 - SL IN 24 |  |  |
SL OUT | SL OUT 25 - BIT1 to SL OUT 48 - BIT16 | SL OUT 25 - SL OUT 48 | *1

*1Write disable

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms