### Settings of External Device

Use the ladder software for communication settings. (Check the operation in CIMPLICITY Machine Edition V4.50)

1. Select "Add Target" -> "GE Fanuc PLC" among "Project" of tool bar and select the series to be connected.
   The selected series is added as "Target" in the project.

2. Allocate the power supply module, the CPU module and the link I/F module in "Hardware Configuration" -> "Main Rack" of added Target.

   NOTE

   - The Rack number and Slot number to allocate by environment using are different.
     Check the environment, and allocate the Rack number and Slot number.

3. Double-click the CPU module and the link I/F module, display the setting window.

4. Set the communication settings.

5. Forward the communication settings to the External Device and spend a power supply of the External Device again.

##### Setup Items

- CPU module

[Settings] tab

Setup Items | Setup Description
--- | ---
SNP ID | 1

- Link I/F module

[Settings] tab

Setup Items | Setup Description
--- | ---
Configuration Mode | SNP Only

[Port1] tab

Setup Items | Setup Description
--- | ---
SNP Enable | Yes
SNP Mode | Slave
Data Rate [bps] | 19200
Parity | Odd
Stop Bits | 1
Flow Control | None

NOTE

- Please refer to the manual of the ladder software for more detail on other setting description.

NOTE

- When using IC693CMM311, select SNP-X protocol for the programming console, and the External Device's WYE cable is necessary. Both Port1 and Port2 can be used as RS-232C connection, and only Port2 can be used as RS-485 connection. When Port2 is used, programming console is needed to select RS-232C or RS-485 connection.
- When using IC697CMM711, select SNP-X protocol for the programming console, and change the interface of Port1/Port2 to RS-232C or RS-485.