### Setting of External Device

Double-click [I/O Table] in the project window to display the [PC I/O Table] window. Select [Unit Settings] from the menu displayed by right-clicking on the Ethernet unit in the window to select the Ethernet Unit Setting Screen.

Setup Items | Setup Description
--- | ---
IP Address Conversion | IP Address Table Method
IP Address Table | Node address and IP address you set in the Display.
IP Address Setting Rotary Switch*2 | 192.168.0.1
Source Network Address*1 | 0
Node Address Setting Rotary Switch*2 | 1
Unit No. Setting Rotary Switch*2 | 0
FINS/UDP Port | 9600

*1Parameter used when you access beyond network.
Set in the routing table of "CX-Net Network Configuration". Please refer to the manual of the External Device for more details.

*2Set with the rotary switch on the front of the Ethernet unit.

##### Notes

- Check with a network administrator about IP address and subnet mask. Do not set the duplicate IP address.

- Always perform the same settings for the port No. of the Display and the External Device.